Below – Left is JDM STI AF481-7546, centre is EU STI, right is S202.
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Below - Left hand side top two are from EU STI, bottom from JDM STI. Right two are from S202.
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