00007A96-7AB5  RPM Points for MIVEC

00007A64-7A8A  Load Points for MIVEC

00006EC8-6EEE  Load Points for Fuel

00006EA0-6EBC  RPM Points for Fuel

00006EFA-6F20  RPM Points for Ignition

00006F2C-6F54  Load Points for Ignition

000031D4-31DA  Injector Battery Compensation

00003277-3285  Accel Enrichment

00001106-1107 Hx00 85= 513cc     Injector size scaling  2 X 1  

000011AA-11AB  Min Coolant Temp for Closed Loop Operation 2 X 1

00001E34-1E36  Hi Intake Temp ISCv step increase A/C on  2 X 1

00001E37-1E38  Hi Intake Temp ISCV Step increase A/C off 2 X 1

00001E30-1E31  Hi Intake Temp ISVC target idle speed A/C on  2 X 1

00001E32-1E33  Hi Intake Temp ISVC target idle speed A/C off 2 X 1

0003FFCE - 3FFCF   Immobilzer code

0000119A  2X1  00 28  OverBoost Delay Timer

00001670  2X1  00 80  Boost Control Load Offset

00002798  2X1  00 A0  Stationary Rev limit

00001180 2X1  03 DA  Rev limit / Formula: 7500000/value= 7606

00002DBD - 2EE8  High Octane Fuel Map

00002EF5 - 3020    Low Octane Fuel Map

000033E9 - 358C    High Octane Ignition Map #1

00003599 - 373C    Low Octane Ignition Map # 1

00005523 - 56C6    High Octane Ignition Map #2

000056D3 - 5876    Low Octane Ignition Map # 2

00005A33 - 5BD6    High Octane Ignition Map # 3

00005BE3 - 5D86    Low Octane Ignition Map # 3

